SMA 公头弯式 接 RG316 线鼻 接线端子
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NOTES |
1. REQUIRMENTS:
1.1. THE PART SHALL BE COMPLIANT WITH
'ROHS DIRECTIVE 2002/95/EC.
1.2. THE CABLE SHALL BE COMPLIANT WITH
IPC/WHMA-4-620 CLASS Il STANDARD.
1.3. THE CABLE SHOULD INCLUDE A WHITE POLYESTER
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LABEL WITH PRINTED PIN, REV. i
1.4. MIN. TEMPERATURE RANGE -25° C T0 +85° C J
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RF convial cable RG316

1.5. VSWR =<1.3:1 1 1

SHA Type nate R/A connectar

2. TESTING: Itemref | Quantity | Titie/Name, designation, material, dimension etc Articie No./Reference
2.2, PULL OUT FORCE 8Kg MINIMUM Vgt | Smenge | hororua ™| ooy 2ronzs | 1

2.3. 100% OPEN, SHORT & MISS WIRE TEST. " 18500320016001

Sheet
"

(@ XAHONOR Scen-echCo,L o S

2.4. INSULATION 300V, 90LC.





